**S2091 Steam Solenoid Valve**

S2091 Series Steam Solenoid Valves are 2/2 way, direct acting, normally closed, high temperature steam solenoid valve. It has Viton diaphragm.

S2091 steam solenoid valves are used in industrial ironing machines with hot water and steam, steam boilers and textile industries.

It is recommended to use solenoid valves with filters. If there are particles such as sand and dirt in the fluid, these will clog the valve and shorten the life of the valve.

In case of malfunction or maintenance, you can get original TORK brand spare parts from our company.

|  |  |  |
| --- | --- | --- |
| **Application** | **:** | Steam, hot water |
| **Size** | **:** | 3/8", 1/2"  |
| **Working Pressure** | **:** | 0…6 Bar (It varies according to orifice) |
| **Core Tube** | **:** | Stainless |
| **Body** | **:** | Brass |
| **Seal** | **:** | Viton, on request EPDM |
| **Fluid Temperature** | **:** | -10°C…160 °C |
| **Position** | **:** | Normally closed |
| **Coil Voltage** | **:** | 230V, 110V, 48V, 24V, 12V  AC; 110V, 48V, 24V, 12 V DC |
| **Protection Class** | **:** | IP65  (on request exproof ) |